





**Practical No-10**

**Configure and test the audio**












**Select option as device registration** 



Register the model




**Download Credentials** 

**Skip this step**





**Do this commands on Respberry Pi cmd**

Generate Credentials 